#### AndroCom: Communication Without Internet

#### Wasia BCS203233

#### Muhammad Harris BCS203193

#### Umer Ahmed BCS203182



**Fall - 2023**

**Supervised By**

**Mr. Bilal Ahmed**

**Department of Computer Science**

**Capital University of Science & Technology, Islamabad**

|  |  |  |
| --- | --- | --- |
|  | Submission Form for Final-Year  PROJECT REPORT |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Version** | | V 2 | |  | **NUMBER OF MEMBERS** | 3 |
|  | | | | | | |
| **TITLE** | AndroCom – Communication without Internet | | | | | |
|  | | | | | | |
| **SUPERVISOR NAME** | | | Mr. Bilal Ahmed | | | |

|  |  |  |
| --- | --- | --- |
| **MEMBER NAME** | **REG. NO.** | **EMAIL ADDRESS** |
| Umer Ahmed | BCS203182 | [Umerahmed1000@gmail.com](mailto:Umerahmed1000@gmail.com) |
| Muhammad Harris | BCS203193 | [Harris20014@gmail.com](mailto:Harris20014@gmail.com) |
| Wasia | BCS203233 | [Wasiaibrar9892@gmail.com](mailto:Wasiaibrar9892@gmail.com) |

|  |  |  |
| --- | --- | --- |
| **MEMBERS’ SIGNATURES** |  | |
|  |  | **Supervisor’s Signature** |
|  |  |
|  |  |

**APPROVAL CERTIFICATE**

This project, entitled as “AndroCom – Communication without Internet” has been approved for the award of

**Bachelors of Science in Computer Science**

**Committee Signatures:**

Supervisor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Mr. Bilal Ahmed)

Project Coordinator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Mr. Bilal Ahmed)

Head of Department: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Dr. Abdul Basit)

**DECLARATION**

*I/We, hereby, declare that “No portion of the work referred to, in this project has been submitted in support of an application for another degree or qualification of this or any other university/institute or other institution of learning”. It is further declared that this undergraduate project, neither as a whole nor as a part thereof has been copied out from any sources, wherever references have been provided.*

|  |
| --- |
| **MEMBERS’ SIGNATURES** |
|  |
|  |
|  |

**ACKNOWLEDGEMENTS**

We express our deepest gratitude to Allah Almighty for granting us the ability to successfully complete this project. Furthermore, we extend our heartfelt appreciation to our parents for their unwavering support and valuable guidance, which has been crucial in various phases of the project's completion. We would like to express our sincere gratitude to Mr. Bilal Ahmed, our supervisor, for their invaluable guidance and support throughout this project. His insightful suggestions and instructions have been pivotal throughout the project.

**Executive Summary**

AndroCom is an innovative communication solution designed to address the challenges posed by limited or no internet access scenarios. In today's interconnected world, where traditional communication methods heavily rely on internet connectivity, AndroCom stands out by providing users with the ability to send text messages, make voice calls, and engage in video calls using a secure, end-to-end encrypted Android app. The uniqueness of AndroCom lies in its offline functionality, enabled through an AD HOC network created by a Raspberry Pi. This approach ensures secure and efficient communication even in situations with no internet connection. The app caters to a wide range of scenarios, including emergency services, disaster recovery, and temporary gatherings, making it a versatile and valuable tool. With a focus on data privacy, security, and global accessibility, AndroCom represents a significant contribution to communication technology, offering users a reliable alternative in challenging connectivity situations.

**Table of Contents**

[Chapter 1 Introduction 11](#_Toc164847845)

[1.1 Project Introduction 11](#_Toc164847846)

[1.2 Existing Examples / Solutions 11](#_Toc164847847)

[1.3 Business Scope 12](#_Toc164847848)

[1.4 Useful Tools and Technologies 12](#_Toc164847849)

[1.5 Project Work Breakdown 14](#_Toc164847850)

[1.6 Project Timeline 15](#_Toc164847851)

[Chapter 2 Requirement Specification and Analysis 16](#_Toc164847852)

[2.1 Functional Requirements 16](#_Toc164847853)

[2.2 Non-Functional Requirements 17](#_Toc164847854)

[2.3 Selected Functional Requirements 17](#_Toc164847855)

[2.4 System Use Case Modeling 18](#_Toc164847856)

[2.5 System Sequence Diagrams 28](#_Toc164847857)

[2.6 Domain Model 36](#_Toc164847858)

[2.7 System Architecture 37](#_Toc164847859)

[Chapter 3 System Design 39](#_Toc164847860)

[3.1 Layer Definition 39](#_Toc164847861)

[3.1.2 Application Layer 39](#_Toc164847862)

[3.1.2 Network Layer 39](#_Toc164847863)

[3.2 Software Architecture 40](#_Toc164847864)

[3.3 Data Flow Diagram 41](#_Toc164847865)

[3.4 User Interface Design 42](#_Toc164847866)

[Chapter 4 Software Development 50](#_Toc164847868)

[4.1 Coding Standards 50](#_Toc164847869)

[4.2 Development Environment 51](#_Toc164847870)

[4.2.1 Tools & Technologies 51](#_Toc164847871)

[4.2.2 Deployment of Development Environment 51](#_Toc164847872)

[4.2.3 Packages and Libraries 52](#_Toc164847873)

[4.3 Software Description 52](#_Toc164847874)

[Chapter 5 Software Testing 64](#_Toc164847876)

[5.1 Testing Methodology 64](#_Toc164847877)

[5.2 Testing Environment 64](#_Toc164847878)

[5.3 Test Cases 65](#_Toc164847879)

[Chapter 6 Software Deployment 72](#_Toc164847876)

[6.1 Installation/Deployment Process Description 72](#_Toc164847877)

[6.1.1 RaspberryPi Setup 72](#_Toc164847878)

[6.1.2 Android Application 74](#_Toc164847878)

[References 77](#_Toc164847876)

**List of Figures**

[**Figure 1.1: Project Work Breakdown** 14](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 1.2: Project Time Line** 15](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.1: System Use Case Diagram** 18](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.2: Establishing Connection With Microcontroller** 28](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.3: Use Profile Setup** 29](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.4: Sharing Active User Pool With User** 30](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.5: Mute User Notification** 31](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.6: Block or Unblock Other Users** 32](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.7: Send Text Messages to Other Users** 33](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.8: Making Voice Call** 34](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.9: Making Video Call** 35](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.10: Domain Model** 36](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.11: System Design** 37](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 2.12: System Architecture** 38](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.1: Software Architecture Diagram** 40](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.2: Data Flow Diagram** 41](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.3: Splash Screen** 42](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.4: Screen Upon Initial Launch** 42](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.5: Profile Setup** 43](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.6: Profile Setup (Filled)** 43](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.7: Chats Screen** 44](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.8: Call Log** 45](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.9: Settings Menu** 46](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.10: Message Screen** 47](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.11: Other User’s Profile View** 48](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.12: Incoming Voice Call Screen** 49](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.13: Ongoing Voice Call Screen** 49](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 3.14: Ongoing Video Call Screen** 49](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188877)

[**Figure 6.1: Terminal in RaspberianOS** 72](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 6.2: Successfully Establishing Ad Hoc Network** 73](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 6.3: Thonny IDE in RaspberryPi** 73](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 6.4: Wireless Debugging in Android Settings** 74](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 6.5: Android Studio** 75](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Figure 6.6: AndroCom App in Android Device** 76](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188877)

**List of Tables**

[**Table 2.1: Functional Requirements** 16](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.2: Non Functional Requirements** 17](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.3: Selected Functional Requirements** 17](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.4: Use Case 1** 19](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.5: Use Case 2** 20](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.6: Use Case 3** 21](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.7: Use Case 4** 22](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.8: Use Case 5** 23](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.9: Use Case 6** 24](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.10: Use Case 7** 25](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.11: Use Case 8** 26](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 2.12: Use Case 9** 27](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 3.1: Layer Definition** 39](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 5.1: Test Case 1** 65](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 5.2: Test Case 2** 66](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 5.3: Test Case 3** 67](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 5.4: Test Case 4** 68](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 5.5: Test Case 5** 69](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 5.6: Test Case 6** 70](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

[**Table 5.7: Test Case 7** 71](file:///D:\Github\Repository\AndroCom\Documentation\Draft%202%20-%20Chapter%201%20to%20Chapter%203.docx#_Toc150188876)

# Chapter 1 Introduction

## Project Introduction

In today's world, the internet has become such an integral part of our lives that if it were to go down tomorrow, most forms of communication, such as messaging, calls, and video communication, would cease to function. AndroCom is an Android app that enables its users to send text messages, make voice calls, and engage in video calls with complete end-to-end encryption when communicating with other users without the need of an internet connection.

AndroCom has significant market potential due to its unique features. It can work in places with no internet, help universities with daily tasks, and serve as a reliable backup during internet outages or emergencies. Its versatility and special capabilities make it valuable in various situations, making it an important tool in the market.

This functionality is implemented through an AD HOC network that is created using a microcontroller, specifically a Raspberry Pi, which serves as a critical component of the system. A server is created on the Raspberry Pi using Python, enabling packet transfer between the Raspberry Pi and the devices using AndroCom. This innovative setup ensures secure and efficient communication while bypassing the need for a traditional internet connection, addressing the challenges posed by internet interruptions or limited access scenarios.

## Existing Examples / Solutions

At present, a noticeable gap exists in the market for apps that offer communication functionality independent of an internet connection. AndroCom, by enabling text messaging, voice calls and video calls with end-to-end encryption using Raspberry Pi, distinguishes itself as an innovative solution that fills this void. Unlike conventional applications that rely on internet connectivity, AndroCom offers users a novel approach to communication in scenarios where such connectivity may be unavailable or limited, addressing a critical need in today's interconnected world.

## Business Scope

The business scope of AndroCom is promising, offering a unique solution for communication in scenarios with limited or no internet access. It caters to a niche market and educational institutions, presents a valuable tool for disaster recovery and emergency services, and has the potential to serve as a backup communication service during internet outages. With its AD HOC networking capabilities, it can find use in various temporary gathering scenarios. The app's focus on data privacy and security also appeals to users prioritizing secure communication, while its potential global reach ensures a broad user base.

## Useful Tools and Technologies

Following is a list of technologies that are used for designing, development and testing phases of the project:

1. **Programming Languages:**
   * **Bash:** Bash is a type of shell scripting language for Unix-based operating systems. It's used to execute commands from the command line and automate tasks.
   * **Kotlin:** Kotlin is a general-purpose programming language initially developed by JetBrains for the Android platform. It's known for being concise, interoperable with Java, and supporting functional programming features.
   * **Java:** Java is a general-purpose, class-based, object-oriented programming language that is widely used for developing applications of various kinds. It's known for its platform independence and code reusability.
   * **Python:** Python is a general-purpose, interpreted, high-level programming language that's known for its readability and ease of use. It's widely used for web development, data science, scripting, and more.
2. **Markup Language:**
   * **XML:** XML is a markup language designed for encoding documents in a machine-readable format. It's used for data interchange between applications and for configuring settings in software programs.
3. **Database:**

* **SQLite:** SQLite is a relational database management system (RDBMS) that is embedded directly into the application. It's a lightweight, self-contained, open-source database that doesn't require a separate server process.

1. **Development Tools:**
   * **Android Studio:** Android Studio is an integrated development environment (IDE) specifically built for Android app development. It provides a comprehensive set of tools for designing, developing, testing, and debugging Android apps.
   * **Thonny IDE:** Thonny is a free and open-source Python IDE designed for beginners. It provides a user-friendly interface with features like syntax highlighting, code completion, and debugging tools.
   * **IntelliJ IDEA:** IntelliJ IDEA is an IDE from JetBrains that supports various programming languages, including Java and Kotlin. It offers a wide range of features for development, testing, and debugging applications.
2. **Design Tool:**
   * **Figma:** Figma is a web-based design tool used for creating user interfaces and user experiences for web and mobile applications.
3. **Hardware:**
   * **Raspberry Pi:** Raspberry Pi is a series of small single-board computers, it's a popular platform for hobbyists and makers due to its affordability and wide range of capabilities.


In our application development, we will employ a hybrid approach, primarily utilizing Kotlin for its modern features and conciseness, while also integrating Java where necessary for specific algorithms, socket programming and several modules. Android Studio will serve as our development environment of choice, offering a comprehensive set of tools for efficient coding and testing. Notably, our app will not rely on an internet connection due to its offline functionality. An AD HOC network is created using Raspberry Pi with a server implemented in Python and Bash.

## Project Work Breakdown

A project work breakdown diagram is a way to break down a complex project into smaller, more manageable tasks. The project work breakdown for the AndroCom is given in *Figure 1.1*.

**Figure 1.1: Project Work Breakdown**

## Project Timeline

A project timeline diagram is a visual representation of the tasks and milestones in a project, showing their start and end dates. In simple words, it's a bar chart that shows when things need to happen in order for your project to finish on time. The project timeline for AndroCom is given in *Figure 1.2*.

**Figure 1.2: Project Time Line**

# 

# Chapter 2 Requirement Specification and Analysis

This chapter documents the specification and analysis of requirements for *AndroCom*. We have systematically sorted out the development requirements for the software, emphasizing the importance of identifying every small detail at this stage to prevent future software alterations.

This chapter covers the following specifications for the required software:

* Functional & Non-Functional Requirements
* Use Case Diagram
* Brief Description of Each Use Case
* Detailed Sequence Diagram for Each Use Case
* Domain Model
* System Architecture

## 2.1 Functional Requirements

Functional requirements are what a system must do to meet user needs. The functional requirements for AndroCom are given in *Table 2.1*.

**Table 2.1: Functional Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
| **S. No.** | **Functional Requirement** | **Type** | **Status** |
| 1 | Configured microcontroller for network connection | Core | Complete |
| 2 | User profile setup in application | Core | Complete |
| 3 | List of active users connected with the network | Core | Complete |
| 4 | Block or unblock users | Intermediate | Incomplete |
| 5 | Mute messages and chat notifications of users | Intermediate | Incomplete |
| 6 | Text Messages with active users | Core | Complete |
| 7 | Voice Calls with active users | Core | Complete |
| 8 | Video Calls with active users | Core | Incomplete |
| 9 | Mute mic or turn-off camera when in call | Intermediate | Incomplete |

## 2.2 Non-Functional Requirements

Non-functional requirements are the constraints on how a system should work. The non-functional requirements for AndroCom are given in *Table 2.2.*

**Table 2.2: Functional and Non-Functional Requirement**

|  |  |  |
| --- | --- | --- |
| **S. No.** | **Non-Functional Requirements** | **Category** |
| 1 | Prompt when connected to the wrong network | Security |
| 2 | De-authorize unauthorized users | Security |
| 3 | End-to-End text encryption | Security |
| 4 | User friendly UI | Usability |
| 5 | View last seen time in active users list | Usability |
| 6 | View Signal Strength with network | Performance |
| 7 | Optimize resource usage on Microcontroller | Performance |
| 8 | Low consumption and Lightweight application | Performance |


## Selected Functional Requirements

The Selected function requirements of AndroCom for FYP Part-II are given in *Table 2.3.*

**Table 2.3: Selected Functional Requirement**

|  |  |  |
| --- | --- | --- |
| **S. No.** | **Functional Requirement** | **Type** |
| 1 | Block or unblock users | Intermediate |
| 2 | Mute message or call notifications of users | Intermediate |
| 3 | Voice Calls with active users | Core |
| 4 | Video Calls with active users | Core |
| 5 | Mute mic or turn off Camera within call | Intermediate |

## System Use Case Modeling

**A system use case diagram is a visual representation of the different ways that users can interact with a system. The system use case diagram of AndroCom is shown in *Figure 2.1.*

**Figure 2.1: System Use Case Diagram**

**Use Case 1 (Configured Microcontroller for Network Connection):**

**Table 2.4: Use Case 1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC1 | | | | |
| **Use Case Name:** | Configured Microcontroller for network connection | | | | |
| **Created By:** | Wasia | | **Last Updated By:** | | Muhammad Harris |
| **Date Created:** | 22-10-2023 | | **Last Revision Date:** | | 29-10-2023 |
| **Actors:** | | User | | | |
| **Description:** | | The user will turn on the microcontroller and connect with its network on his android device | | | |
| **Trigger:** | | The user wants to create an ad hoc network | | | |
| **Preconditions:** | | The user has no internet and wants to use AndroCom for his communication | | | |
| **Post conditions:** | | An ad hoc network will be created via the microcontroller | | | |
| **Normal Flow:** | | User | | System | |
| 1.User turns on the microcontroller | | Microcontroller creates an ad hoc network | |
|  | | 2.User connects with ad hoc network via his android device | | User is connected with the network and is allowed to communicate on the network | |
| **Alternative Flows:** | | None | | | |
| **Exceptions:** | | 1. Microcontroller doesn’t turn on.  2. No network is created by the microcontroller.  3. Network doesn’t show on available networks list. | | | |

**Use Case 2 (User Profile Setup):**

**Table 2.5: Use Case 2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC2 | | | | |
| **Use Case Name:** | User profile setup | | | | |
| **Created By:** | Umer Ahmed | | **Last Updated By:** | | Wasia |
| **Date Created:** | 22-10-2023 | | **Last Revision Date:** | | 30-10-2023 |
| **Actors:** | | User | | | |
| **Description:** | | The user will be presented with a sign-up screen where he enters their first name, last name and optionally uploads their profile picture in app. | | | |
| **Trigger:** | | The user installs the application and wishes to complete their profile setup. | | | |
| **Preconditions:** | | The user has successfully installed the application and is on the initial sign-up screen. | | | |
| **Post conditions:** | | The user’s profile information is saved and he can access, use their profile within application. | | | |
| **Normal Flow:** | | User | | System | |
| 1.User clicks get started button to request for sign-up. | | The system provides a User initial page for profile setup. | |
|  | | 2.User provide first name, last name and clicks continue. | | The system re-direct the User to a newly created profile page. | |
| **Alternative Flows:** | | The user cancels the profile setup. | | | |
| **Exceptions:** | | 1. The User has not filled the form correctly.  2. The system is not responding. | | | |

**Use Case 3 (List of active users connected with network):**

**Table 2.6: Use Case 3**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC3 | | | | |
| **Use Case Name:** | List of active users connected with network | | | | |
| **Created By:** | Wasia | | **Last Updated By:** | | Umer Ahmed |
| **Date Created:** | 22-10-2023 | | **Last Revision Date:** | | 30-10-2023 |
| **Actors:** | | User | | | |
| **Description:** | | System will provide a list of active users who are currently connected to the network for monitoring and management purposes. | | | |
| **Trigger:** | | The user selects the “Active Users” option from the application menu. | | | |
| **Preconditions:** | | User is logged into the application and a connection is established. | | | |
| **Post conditions:** | | The application displays a list of all active users connected to the network. | | | |
| **Normal Flow:** | | User | | System | |
| 1. The user selects the “Active Users” option from the application menu. | | The system displays the list of active users to the user. | |
| **Alternative Flows:** | | Network connection is not established and error message will be displayed. | | | |
| **Exceptions:** | | Network server is unavailable. | | | |

**Use Case 4 (Text messages with active users):**

**Table 2.7: Use Case 4**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC4 | | | | |
| **Use Case Name:** | Text messages with active users | | | | |
| **Created By:** | Muhammad Harris | | **Last Updated By:** | | Wasia |
| **Date Created:** | 22-10-2023 | | **Last Revision Date:** | | 30-10-2023 |
| **Actors:** | | User | | | |
| **Description:** | | User can send and receive text messages to other active users on the network. | | | |
| **Trigger:** | | The user selects the chat icon from the application menu. | | | |
| **Preconditions:** | | The user must be connected to network and is logged into the application. | | | |
| **Post conditions:** | | The user is able to send and receive text messages to other active users on a network. | | | |
| **Normal Flow:** | | User | | System | |
| 1. The user selects the chat icon from application menu. | | The system displays the chat section the application. | |
|  | | 2.The user selects the recipient of a text message. | | The system highlights selected recipient. | |
|  | | 3. The user enters the text message and sends it. | | The system send text message to the recipient over network. | |
| **Alternative Flows:** | | Recipient is not active and text message is not delivered. | | | |
| **Exceptions:** | | 1. User not logged into the application  2. Network server is unavailable. | | | |

**Use Case 5 (Block or unblock users):**

**Table 2.8: Use Case 5**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC5 | | | | |
| **Use Case Name:** | Block and unblock users | | | | |
| **Created By:** | Umer Ahmed | | **Last Updated By:** | | Wasia |
| **Date Created:** | 22-10-2023 | | **Last Revision Date:** | | 30-10-2023 |
| **Actors:** | | User | | | |
| **Description:** | | User can block and unblock other user within application. Blocking user will prevent further communication from or to the blocked user. | | | |
| **Trigger:** | | The user selects the “Block or unblock users” option from the application menu. | | | |
| **Preconditions:** | | User must be connected to network and is logged into the application interacting with the user whose status they want to change. | | | |
| **Post conditions:** | | The selected user is either blocked or unblocked, as per the user’s action. | | | |
| **Normal Flow:** | | User | | System | |
| 1. The user selects the “Block or unblock users” from application menu. | | The system displays a list of all active users on the network. | |
|  | | 2.The user selects the user they want to block or unblock. | | The system blocks or unblocks the selected user. | |
| **Alternative Flows:** | | User is already blocked or selected user is not active. | | | |
| **Exceptions:** | | 1. User not logged into the application.  2.Network connection is not established. | | | |

**Use Case 6 (Voice call with active users):**

**Table 2.9: Use Case 6**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC6 | | | | |
| **Use Case Name:** | Voice call with active users | | | | |
| **Created By:** | Umer Ahmed | | **Last Updated By:** | | Muhammad Harris |
| **Date Created:** | 10-10-2023 | | **Last Revision Date:** | | 11-10-2023 |
| **Actors:** | | User | | | |
| **Description:** | | User can initiate and receive a voice call from an active user within application. | | | |
| **Trigger:** | | The user will press the call icon from the text chat section. | | | |
| **Preconditions:** | | User must be connected to network and is logged into the application. The user has selected an active user from the list and indicated to make a voice call. | | | |
| **Post conditions:** | | The user is able to a voice call with another active user on the network. | | | |
| **Normal Flow:** | | User | | System | |
| 1. The user selects the recipient of the voice call and initiates the voice call. | | The system sends a voice call request to the recipient over the network. | |
|  | | 2. The users are able to talk to each other over the voice connection. | | The system establishes a voice connection between two users. | |
| **Alternative Flows:** | | The recipient user rejects the voice call request and call is not established. | | | |
| **Exceptions:** | | 1. User not logged into the application.  2.Selected active user is no longer available or active. | | | |

**Use Case 7 (mute messages and call notifications of users):**

**Table 2.10: Use Case 7**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC7 | | | | |
| **Use Case Name:** | Mute messages and call notifications of users | | | | |
| **Created By:** | Wasia | | **Last Updated By:** | | Muhammad Harris |
| **Date Created:** | 10-10-2023 | | **Last Revision Date:** | | 19-10-2023 |
| **Actors:** | | User | | | |
| **Description:** | | User can mute messages and call notifications of specific users within application. | | | |
| **Trigger:** | | The user selects the “Mute messages and call notification” option from the settings or user preferences section. | | | |
| **Preconditions:** | | User must be connected to network and is logged into the application. Also, user has identified specific users from whom they want to mute notifications. | | | |
| **Post conditions:** | | The selected user’s message and call notifications are either muted or unmuted, as per user’s action. | | | |
| **Normal Flow:** | | User | | System | |
| 1. The user selects the “Mute messages and call notifications” option. | | The system displays a list of all active users on the network. | |
|  | | 2. The user selects the users whose messages and call notifications they want to mute. | | The system mutes messages and call notifications from the selected user. | |
| **Alternative Flows:** | | The selected user is already muted or a user is not active. | | | |
| **Exceptions:** | | 1. User not logged into the application and is not connected to the network. | | | |

**Use Case 8 (Video call with active users):**

**Table 2.11: Use Case 8**


|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC8 | | | | |
| **Use Case Name:** | Video call with active users | | | | |
| **Created By:** | Wasia | | **Last Updated By:** | | Muhammad Harris |
| **Date Created:** | 21-4-2024 | | **Last Revision Date:** | | 25-4-2024 |
| **Actors:** | | User | | | |
| **Description:** | | User can initiate and receive a video call from an active user within application. | | | |
| **Trigger:** | | The user will press the video call icon from the text chat section. | | | |
| **Preconditions:** | | User must be connected to network and is logged into the application. The user has selected an active user from the list and indicated to make a video call. | | | |
| **Post conditions:** | | The user is able to make a video call with another active user on the network. | | | |
| **Normal Flow:** | | User | | System | |
| 1. The user selects the recipient of the video call and initiates the video call. | | The system sends a video call request to the recipient over the network. | |
|  | | 2. The users are able to talk to each other over the video connection. | | The system establishes a video connection between two users. | |
| **Alternative Flows:** | | The recipient user rejects the video call request and call is not established. | | | |
| **Exceptions:** | | 1. User is not logged into the application.  2. Select active user. | | | |

**Use Case 9 (Mute mic or turn-off camera):**


**Table 2.12: Use Case 9**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Use Case ID:** | UC9 | | | | |
| **Use Case Name:** | Mute mic and turn-off the camera | | | | |
| **Created By:** | Umer Ahmed | | **Last Updated By:** | | Muhammad Harris |
| **Date Created:** | 21-4-2024 | | **Last Revision Date:** | | 25-4-2024 |
| **Actors:** | | User | | | |
| **Description:** | | User mutes their microphone and turn-off the camera to avoid unwanted noise and to maintain focus on call content. | | | |
| **Trigger:** | | The user will press the mute mic and turn-off the camera icon on the call screen. | | | |
| **Preconditions:** | | The user must be connected to the network and is logged into the application. The user is participating in a call. | | | |
| **Post conditions:** | | The user’s microphone and camera can be independently muted or turned off, and no audio or video is transmitted by the user’s device. | | | |
| **Normal Flow:** | | User | | System | |
| 1. The user decides to mute the microphone or turn-off the camera. | | The system provides both microphone mute and turn-off camera buttons to the user. | |
|  | | 2. The user either clicks the mute or turn-off camera button. | | The system confirms the actions of user. | |
| **Alternative Flows:** | | The user clicks the mute or turn-off camera button but the microphone remains unmuted and the camera isn’t turned off. | | | |
| **Exceptions:** | | The call with another user crashes and the mute mic or turn off camera functionality becomes unavailable. | | | |


## System Sequence Diagrams

A system use case sequence diagram is a visual representation of the steps involved in a particular use case of a system, showing the interactions between the different actors and components of the system. Following are the sequence diagrams for AndroCom application.


**Figure 2.2: Establishing connection with microcontroller**




**Figure 2.3: User profile setup**




**Figure 2.4: Sharing active user pool with user**




**Figure 2.5: Mute user notifications**




**Figure 2.6: Block or Unblock other users**




**Figure 2.7: Send text message to other users**



**Figure 2.8: Making a voice call**

**Figure 2.9: Making a Video call**

## Domain Model

A domain model is a conceptual map of the key concepts and relationships in a problem domain. Domain models are used to help developers understand and design software. The domain model for AndroCom is given below in *figure 2.10.*


**Figure 2.10: Domain Model**

## 2.7 System Architecture


The system architecture of AndroCom is designed to provide a reliable and secure way for users to communicate without an internet connection. The system consists of a client app and a microcontroller. The client app is responsible for establishing a connection to the AD HOC network, sending and receiving messages, and making and receiving voice and video calls. The microcontroller is responsible for managing the AD HOC network and relaying messages between clients. The microcontroller is very portable and can be attached to transport vehicles and drones.

The client app and the server communicate with each other using TCP/IP sockets. The server also uses UDP sockets to broadcast messages to all clients on the AD HOC network.

The system architecture and system design are shown in *figure 10.11* and *figure 10.12.*



**Figure 2.11: System Design**



**Figure 2.12: System Architecture**

# Chapter 3 System Design

The purpose of this chapter is to provide information that is complementary to the code. Without an adequate design that delivers required function as well as quality attributes, the project will fail. But communicating architecture to its stakeholders is as important a job as creating it in the first place.

This chapter covers the following specifications for the required software:

* Layer Definition
* Software Architecture
* Data Flow Diagram
* User Interface Design

## 3.1 Layer Definition

A layer definition is a description of the purpose, functionality, and interfaces of a layer in a layered system. In simple words, it is a definition of what a layer does and how it interacts with other layers. Layer definition for AndroCom is given in *Table 3.1.*

**Table 3.1: Layer Definition**

|  |  |
| --- | --- |
| **Layers** | **Description** |
| Application Layer (AndroCom App) | This layer is responsible for providing user interfaces and other key functionalities. |
| Network Layer (Microcontroller) | This layer is responsible for communicating with the microcontroller over a network. |


## 3.1.2 Application Layer

This layer is responsible for implementing the core functionality of the application, such as connecting sockets, sending and receiving messages, making & receiving voice and video calls, and interacting with the user interface.

## 3.1.2 Network Layer



This layer is responsible for communicating with the microcontroller over a network. The AndroCom App layer sends and receives messages to and from the network layer. The network layer then sends and receives messages to and from the microcontroller.

## Software Architecture

A software architecture diagram is a visual representation of the structure of a software system, showing the components of the system and how they interact. In simpler words, it is a diagram that shows how a software system is built. The software architecture diagram is given below in *figure 3.1.*

**Figure 3.1: Software Architecture Diagram**

## Data Flow Diagram

**A Data Flow Diagram is a graphical representation of the flow of data through a system, showing its inputs, outputs, and processing steps. The data flow diagram for AndroCom is given in *figure 3.2.*

**Figure 3.2: Data Flow Diagram**

## User Interface Design



****User interface design is the process of creating interactive screens that are easy to use and understand. The UI design for AndroCom is given below.

**Figure 3.4: Screen upon initial launch**

**Figure 3.3: Splash Screen**

**Description:**

The AndroCom app's splash screen is the first thing users see when they open the app. It displays the app's logo in the center against a white background. This screen creates a strong initial impression and sets the stage for the user's interaction with the app.




**Figure 3.6: Profile Setup (filled)**

**Figure 3.5: Profile Setup**

**Description:**

The profile setup screen in AndroCom is where users enter their first name and last name. It's a clean and minimalist design, with input fields for both names. What's distinctive is the 'Next' button, which remains inactive until both fields are filled. This encourages users to provide their information, ensuring a complete profile setup.

****

**Figure 3.7: Chats Screen**


**Description:**

The chat screen in AndroCom is where users can seamlessly engage in multiple conversations. The user-friendly interface allows users to view and manage various chat threads.

**Description:**


**Figure 3.8: Call Log**

The call log screen in AndroCom provides users with a comprehensive record of their recent calls and also displays active users with whom call can be made.

**Description:**

**Figure 3.9: Settings Menu**


The settings screen in AndroCom is where you can easily view and edit your display name, unblock users, activate network prioritization, adjust notification settings, and access the privacy policy and manual.

**Description:**

**Figure 3.10: Message Screen**

The messaging screen in AndroCom is where you can scroll through older messages and send new ones to active users. Also, you can make voice and video calls directly from this screen, ensuring that your communication needs are all in one place.

**Figure 3.11: Other User's Profile View**

**Description:**

When viewing another person's profile in AndroCom, you'll find essential information at a glance. This includes their name and MAC address, making it easy to identify and connect with them. Additionally, you have the option to mute or block the user.

**Description:**

**Figure 3.14: Ongoing Video Call Screen**

**Figure 3.13: Ongoing Voice Call Screen**

**Figure 3.12: Incoming Voice Call Screen**

In AndroCom, when you receive an incoming voice call, the caller's name is prominently displayed. By sliding, you can accept the call. During an ongoing voice call, you have the option to mute your microphone for privacy and convenience. And for video calls, you can mute the microphone or disable the camera.

# Chapter 4

# Software Development

This section provides an in-depth exploration of the software development phase for AndroCom. Here, we systematically outline the key elements that contribute to the creation of a robust and efficient communication application. Emphasizing the importance of precision in this phase to avoid future alterations, we delve into the specifics of our software development approach.

The following components are covered in this section:

* Coding Standards
* Development Environment
* Software Description

## Coding Standards

The following coding standards were followed in development of this project,

* Python
  1. Indentation: Consistent four spaces.
  2. Declaration: Snake\_case for variables (e.g., broadcast\_ip).
  3. Naming Convention: Snake\_case for variables and functions.
  4. Statement Standard: Each statement on a new line, comments for purpose explanations, and a clear function definition.
* Kotlin
  1. Indentation: Four spaces consistently.
  2. Declaration: CamelCase for class and package names (e.g., SendMessage).
  3. Naming Convention: CamelCase for class names, lowercase for package names.
  4. Statement Standard: Each statement on a new line, comments for code structure explanations.

## Development Environment

The tools and technologies used for the development of AndroCom along with critical libraries and packages are given below. Also, the deployment process for development environment is provided as well.

## 4.2.1 Tools & Technologies

The following are the tools and technologies used in the development of AndroCom,

* **Bash (Microcontroller Scripting):** Bash was for creating AD HOC network in the microcontroller, facilitating communication between android application and microcontroller.
* **Python (Microcontroller Side Programming):** Utilized for programming the microcontroller, ensuring efficient execution of tasks on the microcontroller side such as sending IP addresses & MAC addresses of connected devices to android application.
* **Kotlin (Android Application):** Chosen as the primary language for Android application development, providing a robust framework for building user interfaces and implementing functionalities.
* **Thonny IDE (Python on Microcontroller):** Specifically used for Python development on the microcontroller, providing a user-friendly interface and tools for coding, testing, and debugging Python scripts on a Linux operating system.
* **Visual Studio Code (Testing and Logic Development):** Used for testing and logic development, providing a versatile and lightweight integrated development environment (IDE) for multiple coding tasks.
* **Android Studio (Android Application Development):** The major IDE for Android app development, offering comprehensive tools and features for designing, coding, testing, and debugging Android applications.

## 4.2.2 Deployment of Development Environment

The deployment process involved the installation and configuration of the respective development environments on the relevant platforms such as Windows and RaspberrianOS (Linux). Each environment was tailored to suit the specific requirements of the development phase.

## 4.2.3 Packages and Libraries

The following are the two major libraries used in the development of our project,

* **Socket (Python):** It was used for creating UDP packets on microcontroller and sending it over the android application through AD HOC network.
* **Java Socket (Kotlin):** This is the most critical library to our android application. It provided all the necessary functions needed to create the functionality of receiving UDP packets from microcontroller and sending/receiving messages to other devices using TCP/IP Sockets through AD HOC network.

## Software Description

**Snippet 1**

!/bin/bash

# Check if NetworkManager is installed

if ! command -v nmcli &> /dev/null; then

echo "NetworkManager is not installed. Please install it first."

exit 1

fi

# Set your desired network information

NETWORK\_NAME="Ad-HocNetwork"

SSID="Ad-HocNetwork"

PASSWORD="12345678"

#Delete existing connection (if any)

sudo nmcli connection delete "$hotspot\_ssid" 2>/dev/null

# Create a new connection with a /27 subnet

nmcli con add type wifi ifname '\*' con-name $SSID autoconnect yes ssid $SSID 802-11-wireless.mode ap 802-11-wireless.band bg ipv4.method shared

nmcli con modify $SSID 802-11-wireless.security.key-mgmt wpa-psk

nmcli con modify $SSID 802-11-wireless-security.psk $PASSWORD

# Set the network address and subnet mask for a /27 subnet

nmcli con modify $SSID ipv4.addresses "192.168.1.1/27"

# Bring up the WiFi connection

nmcli con up $SSID

# Display the status of the WiFi connection

nmcli con show $SSID | grep GENERAL.STATE

echo "WiFi network '$SSID' with a /27 subnet is now running."

# Function to list connected devices

list\_connected\_devices() {

echo "Connected Devices:"

sudo arp -a | grep "$wifi\_interface" | awk '{print $1, $2}'

}

# Trap to handle SIGINT (Ctrl+C) and list connected devices before exiting

trap 'list\_connected\_devices; exit' SIGINT

# Continuously list connected devices

while true; do

list\_connected\_devices

sleep 10 # Adjust the sleep interval as needed

done

**Description**: This Bash script automates the setup of an AD HOC WiFi network using NetworkManager on a Linux system. It begins by checking for the presence of NetworkManager, prompting the user to install it if necessary. The script then defines network parameters like the network name, SSID, and password, attempting to delete any existing connection with the specified SSID. A new WiFi connection is created with specific settings, including AD HOC mode and a /27 subnet. Security configurations such as WPA-PSK are applied, and the network address and subnet mask are set. The script activates the WiFi connection, displays its status, and continuously lists connected devices using the ARP table.

This script streamlines the process of establishing and managing an AD HOC network, providing real-time information on connected devices. Adjustments to network parameters can be made to suit specific requirements.

**Snippet 2**

import subprocess

import json

import time

import socket

# Specify the broadcast IP address and port

broadcast\_ip = '192.168.1.31' # Replace with the broadcast address of your local network

broadcast\_port = 54321

# Create a socket object for broadcasting

broadcast\_socket = socket.socket(socket.AF\_INET, socket.SOCK\_DGRAM)

broadcast\_socket.setsockopt(socket.SOL\_SOCKET, socket.SO\_BROADCAST, 1)

def get\_connected\_devices():

try:

# Run the arp command and capture its output

result = subprocess.check\_output(['arp', '-a'], universal\_newlines=True)

# Split the output into lines

lines = result.split('\n')

# Extract IP addresses and corresponding MAC addresses

devices = {}

for line in lines:

if 'ether' in line:

parts = line.split()

ip\_address = parts[1]

mac\_address = parts[3]

devices[mac\_address] = ip\_address.strip('()')

return {"devices":devices}

except subprocess.CalledProcessError:

print("Error executing the arp command.")

return None

# Broadcast the JSON string every 2 seconds (for example)

while True:

connected\_devices = get\_connected\_devices()

if connected\_devices:

# Create a JSON object to send

x = json.dumps(connected\_devices, indent=4)

broadcast\_socket.sendto(x.encode(), (broadcast\_ip, broadcast\_port))

print(f"Broadcasted: {x}")

time.sleep(2)

else:

print("Failed to retrieve connected devices.")

# Close the broadcasting socket (this will never be reached in the example)

broadcast\_socket.close()

**Description**: This Python script is programed to discover and broadcast information about connected devices within the AD HOC network. It utilizes the ARP (Address Resolution Protocol) command to retrieve a list of connected devices along with their IP and MAC addresses. The script then packages this information into a JSON object and broadcasts it at regular intervals using a UDP socket. The specified broadcast IP address and port facilitate the dissemination of device information across the network. The loop ensures continuous execution, periodically updating and broadcasting the list of connected devices.

Overall, this script provides a mechanism to dynamically share information about connected devices within the network, serving applications where real-time device presence tracking is essential. Adjustments to the broadcast IP, port, or update frequency can be made based on specific network requirements.

**Snippet 3**

package com.example.androcomtest

import java.net.DatagramPacket

import java.net.DatagramSocket

class activity\_Contacts : AppCompatActivity() {

val callsIcon = findViewById<ImageView>(R.id.callsIcon)

val settingsIcon = findViewById<ImageView>(R.id.settingsIcon)

val callText=findViewById<TextView>(R.id.callText)

val settingText=findViewById<TextView>(R.id.settingText)

val chatText=findViewById<TextView>(R.id.chatText)

val chatIcon = findViewById<ImageView>(R.id.chatIcon)

private lateinit var binding : ActivityMainBinding

private lateinit var userIPArray: ArrayList<UserIP>

private lateinit var listView: ListView

private lateinit var adapter : IPAdapter

override fun onCreate(savedInstanceState: Bundle?) {

super.onCreate(savedInstanceState)

callsIcon.setOnClickListener {

val intent = Intent(this, calls\_activity::class.java)

startActivity(intent)

}

callText.setOnClickListener {

val intent = Intent(this, calls\_activity::class.java)

startActivity(intent)

}

settingText.setOnClickListener {

val intent = Intent(this, activity\_app\_settings::class.java)

startActivity(intent)

}

settingsIcon.setOnClickListener {

val intent = Intent(this, activity\_app\_settings::class.java)

startActivity(intent)

}

chatIcon.setOnClickListener {

val intent = Intent(this, activity\_HomeScreen::class.java)

startActivity(intent)

}

chatText.setOnClickListener {

val intent = Intent(this, activity\_HomeScreen::class.java)

startActivity(intent)

}

binding =ActivityMainBinding.inflate(layoutInflater)

setContentView(binding.root)

userIPArray= ArrayList()

listView=findViewById(R.id.contactlist)

adapter = IPAdapter(this,userIPArray)

listView.adapter=adapter

startIPReceiver()

}

private fun startIPReceiver() {

CoroutineScope(Dispatchers.IO).launch {

try {

val socket = DatagramSocket(54321)

while (true) {

try {

val packet = DatagramPacket(ByteArray(1024), 1024)

socket.receive(packet)

val receivedData = String(packet.data, 0, packet.length)

try {

// Assuming JSON format:

val devices = JSONObject(receivedData)

val newUserIPs = ArrayList<UserIP>()

val devicesJSONObject = devices.getJSONObject("devices")

val deviceKeys = devicesJSONObject.keys()

for (ipKey in deviceKeys) {

val ip = devicesJSONObject.getString(ipKey)

newUserIPs.add(UserIP("username ","userIP $ip"))

}

runOnUiThread {

userIPArray.clear()

userIPArray.addAll(newUserIPs)

adapter.notifyDataSetChanged()

}

} catch (e: JSONException) {

handleInvalidDataError(e)

}

} catch (e: IOException) {

handleNetworkError(e)

}

}

} catch (e: SocketException) {

handleSocketError(e)

}

}

}

private fun handleInvalidDataError(e: JSONException) {

runOnUiThread {

Toast.makeText(this, "Error parsing received data: ${e.message}", Toast.LENGTH\_LONG).show()

}

}

private fun handleNetworkError(e: IOException) {

runOnUiThread {

Toast.makeText(this, "Network error: ${e.message}", Toast.LENGTH\_LONG).show()

}

}

private fun handleSocketError(e: SocketException) {

runOnUiThread {

Toast.makeText(this, "Socket error: ${e.message}", Toast.LENGTH\_LONG).show()

}

}

}

**Description**: This Kotlin code represents an Android activity named activity\_Contacts within the "androcom" application. The main functionality revolves around receiving and processing data from a DatagramSocket which are coming from the microcontroller, presumably containing information about connected devices in the network. The received data, assumed to be in JSON format, is parsed to extract IP addresses and populate a user interface list with UserIP objects. The startIPReceiver function is implemented using Kotlin coroutines to continuously listen for incoming data on a DatagramSocket.

Overall, this code contributes to the creation of a dynamic contact list based on real-time data received from the microcontroller via the AD HOC network, enhancing the communication features of the Android application.

**Snippet 5**

package com.example.androcom

import java.io.BufferedReader

import java.io.InputStreamReader

import java.io.OutputStreamWriter

import java.net.Socket

import android.os.AsyncTask

class activity\_chat : AppCompatActivity() {

lateinit var recyclerView: RecyclerView

lateinit var progressBar: ProgressBar

lateinit var inputMessage: EditText

lateinit var adapter: ChatAdapter

private val handler = Handler(Looper.getMainLooper())

override fun onCreate(savedInstanceState: Bundle?) {

super.onCreate(savedInstanceState)

setContentView(R.layout.activity\_chat)

val textname =findViewById<TextView>(R.id.textname)

val backicon=findViewById<AppCompatImageView>(R.id.backicon)

recyclerView = findViewById(R.id.chatRecyler)

progressBar = findViewById(R.id.progress)

inputMessage = findViewById(R.id.inputmessage)

val sendButton = findViewById<FrameLayout>(R.id.layoutsend)

adapter = ChatAdapter()

recyclerView.adapter=adapter

sendButton.setOnClickListener {

val message = inputMessage.text.toString()

SendTask().execute(message)

inputMessage.setText("")

}

val username = intent.getStringExtra("username")

if (username != null) {

textname.text = username

}

backicon.setOnClickListener{

val intent = Intent(this, activity\_HomeScreen::class.java)

startActivity(intent)

}

}

override fun onResume() {

super.onResume()

ReceiveTask().execute()

}

private inner class ReceiveTask : AsyncTask<Void, String, Unit>() {

override fun doInBackground(vararg params: Void?) {

Recieve\_Message()

}

override fun onProgressUpdate(vararg values: String?) {

// UI updates on receiving messages

val receivedMessage = Message(values[0] ?: "", false)

addMessageToRecyclerView(receivedMessage)

}

}

private fun addMessageToRecyclerView(message: Message) {

// Access your adapter for the RecyclerView

val adapter = recyclerView.adapter as ChatAdapter // Assuming you have a ChatAdapter

adapter.addMessage(message)

recyclerView.smoothScrollToPosition(adapter.itemCount - 1) // Scroll to bottom

}

private inner class SendTask : AsyncTask<String, Void, String>() {

private lateinit var sentMessage: String

override fun doInBackground(vararg params: String): String? {

val message = params[0]

sentMessage = message // Store the message in the class-level variable

Send\_Message(IP\_Address, message)

return null

}

override fun onPostExecute(result: String?) {

// UI updates after sending message

val message = sentMessage // Access the stored message

val sentMessage = Message(message, true)

addMessageToRecyclerView(sentMessage)

}

}

var socket: Socket? = null

fun Send\_Message(IP\_Address: String, Message: String) {

try {

if (socket == null) {

socket = Socket(IP\_Address, 49153)

}

// Use a temporary variable for smart cast

val currentSocket = socket

if (currentSocket != null) {

val writer = OutputStreamWriter(currentSocket.getOutputStream())

writer.write(Message)

writer.flush()

println("Message Sent")

} else {

println("Socket is null")

}

} catch (e: IOException) {

// Handle error

println("Error sending message: $e")

socket?.close() // Close if an error occurs

socket = null

}

}

fun Recieve\_Message() {

try {

// Create server socket

val serverSocket = ServerSocket(49153)

while (true) { // Continuous listening loop

// Accept client connection

val clientSocket = serverSocket.accept()

// Read message

val reader = BufferedReader(InputStreamReader(clientSocket.getInputStream()))

val message = reader.readLine()

println("Received Message: $message")

// Handle message (e.g., display in UI)

handler.post {

addMessageToRecyclerView(Message(message, false))

}

// Close client socket (optional)

clientSocket.close()

}

} catch (e: IOException) {

// Handle error

println("Error receiving message: $e")

}

}

}

**Description**: This Kotlin code defines an Android activity named activity\_chat within the "androcom" application. The activity facilitates real-time chat functionality. The layout includes UI elements such as a RecyclerView for displaying chat messages, a ProgressBar, and an EditText for inputting messages. Additionally, there is a TextView to show the username of the chat, a back icon to navigate to the home screen, and a send button to transmit messages. The RecyclerView is linked to a ChatAdapter for managing and displaying chat messages.

Upon creating the activity, it initializes various UI components and sets up click listeners. It launches an AsyncTask called ReceiveTask in the onResume method, responsible for continuously listening for incoming messages in the background. Received messages are processed in the doInBackground method and updated on the UI using onProgressUpdate.

The SendTask AsyncTask is utilized to handle the process of sending messages. It communicates with the server socket specified by the IP address and port. The Send\_Message function establishes a socket connection, sends the message, and handles potential errors.

The Recieve\_Message function represents the server-side logic for message reception. It continuously listens for client connections, reads incoming messages, and updates the UI with the received message using the addMessageToRecyclerView function.

The overall structure of the code demonstrates a basic chat application with functionalities for sending and receiving messages, and it incorporates asynchronous tasks to handle networking operations in the background. The use of AsyncTask ensures that networking tasks do not block the main UI thread, providing a smoother user experience. Additionally, error handling mechanisms are implemented to manage potential issues during socket operations.

# Chapter 5

# Software Testing

This chapter provides a description of the adopted testing procedure, including the selected testing methodology, unit tests, and the test results of the developed software.

## 5.1 Testing Methodology

We employed black box testing as our chosen testing methodology, leveraging its efficiency and several inherent advantages. Black box testing is a software testing approach that assesses the functionality of an application without delving into its internal structures or workings. This method is versatile and applicable to various levels of software testing, including unit, integration, system, and acceptance testing. Specifically, black box unit testing played a crucial role in our project. Unit testing, a subset of black box testing, evaluates individual units of source code, assessing their fitness for use based on defined criteria.

## 5.2 Testing Environment

We are conducting manual testing by writing test cases for every module. We provide inputs to these test cases and then verify the results of each test case. During the testing phase of AndroCom, a variety of testing environments have been utilized to ensure the thorough evaluation of the application's functionalities.

Emulated environments have provided insights into the application's compatibility across various virtual devices, enabling testing under different screen sizes, resolutions, and Android versions. Real Android devices have been employed to validate the application's real-world performance, uncovering device-specific issues that may not be evident in emulated environments.

The microcontroller setup, including hardware like Raspberry Pi and Python scripts, has been essential for testing the communication and integration between the Android application and the microcontroller. Ad hoc network and network interruption testing environments have been created to assess the application's functionality in scenarios with limited or no internet connectivity, as well as its resilience to network disruptions. This comprehensive testing approach aims to guarantee that AndroCom performs reliably across diverse conditions and scenarios, meeting the expectations of end-users.

## 5.3 Test Cases

**Test Case 1: Verify that the microcontroller successfully creates an AD HOC network**

**Table 5.1: Test Case 1**

|  |  |
| --- | --- |
| Date: 06 December 2023 |  |
| *System:* AndroCom |  |
| *Objective:* Make sure that the created network has the correct SSID, password and network name. Also, the created network should be visible as a Wi-Fi network and devices must be able to connect with it. | *Test ID:* 1 |
| *Version:* 1 | *Test Type:* Unit testing |
| *Input:* SSID, Network Name and Password to Bash script in microcontroller. | |
| *Expected Result:* Created AD HOC network has correct SSID, Network Name and Password. Also, devices are able to connect with the network. | |
| *Actual Result:* Passed | |

**Description**: In this test case, a network was created via the microcontroller using a bash script. The script established a network using an SSID, Network Name, and Password provided within the script. Once the script was executed, the network became visible on all devices with Wi-Fi capability. All devices were able to successfully connect to the network.

**Test Case 2: Ensure that the microcontroller accurately broadcasts the IP and MAC addresses of connected devices**

**Table 5.2: Test Case 2**

|  |  |
| --- | --- |
| Date: 08 December 2023 |  |
| *System:* AndroCom |  |
| *Objective:* Make sure that the microcontroller successfully broadcasts the IP and MAC addresses of connected devices. | *Test ID:* 2 |
| *Version:* 1 | *Test Type:* Unit testing |
| *Input:* Connect device with network. | |
| *Expected Result:* The UDP packet containing IP and MAC addresses was successfully broadcasted by microcontroller to all connected devices. The packet contained correct IP and MAC addresses. | |
| *Actual Result:* Failed | |

**Description**: In this test case, IP and MAC addresses of all connected devices were broadcasted to all android devices. The message was successfully broadcasted by microcontroller and received by the android app. The IP address received was accurate. However, MAC address received did not match the device MAC address.

**Test Case 3: Ensure IP and MAC address logs are updated in real-time**

**Table 5.3: Test Case 3**

|  |  |
| --- | --- |
| Date: 08 December 2023 |  |
| *System:* AndroCom |  |
| *Objective:* Ensure IP and MAC address logs are updated in real-time | *Test ID:* 3 |
| *Version:* 1 | *Test Type:* Unit testing |
| *Input:* ARP Table | |
| *Expected Result:* The log contains the IP address and MAC address of connected devices. The log is updated in real-time in case a device joins or disconnects with the network. | |
| *Actual Result:* Passed | |

**Description**: In this test case, the python script for microcontroller maintained a log of connected devices, with their IP and MAC addresses. The log was real-time and was updated when a device connected or disconnected with the network.

**Test Case 4: Testing the app setup process by entering a full user name**

**Table 5.4: Test Case 4**

|  |  |
| --- | --- |
| Date: 01 December 2023 |  |
| *System:* AndroCom |  |
| *Objective:* Test the app setup process by entering a full user name. Ensure that the application accepts and stores the user name correctly. | *Test ID:* 4 |
| *Version:* 1 | *Test Type:* Unit testing |
| *Input:* First Name and Last Name | |
| *Expected Result:* Once, the user completes the profile setup, his name is stored in the android app and can be viewed in setting. | |
| *Actual Result:* Passed | |

**Description**: In this test case, when the user opens the android application for the first time, he has to setup his profile. This is a onetime process. Once, the enters his first and last name, the continue button appears and user can finish setting up. Null values were not accepted. Entered name was successfully saved and was visible in settings.

**Test Case 5: Verify received IP and MAC addresses on android application**

**Table 5.5: Test Case 5**

|  |  |
| --- | --- |
| Date: 10 December 2023 |  |
| *System:* AndroCom |  |
| *Objective:* Verify that the application correctly displays a list of active devices connected to the microcontroller. This includes checking if the list is updated in real-time as devices connect or disconnect. | *Test ID:* 5 |
| *Version:* 1 | *Test Type:* Unit testing |
| *Input:* UDP Packet sent by microcontroller | |
| *Expected Result:* The android application successfully receives the UDP packet sent by the microcontroller. The app displays IP and MAC addresses in UI. | |
| *Actual Result:* Passed | |

**Description**: In this test case, when the device is connected with the AD HOC network, the user opens the app and checks the connected devices. All the IP and MAC addresses were accurate.

**Test Case 6: Testing that the message is successfully sent by the android app**

**Table 5.6: Test Case 6**

|  |  |
| --- | --- |
| Date: 28 December 2023 |  |
| *System:* AndroCom |  |
| *Objective:* Test the message sending functionality by composing and sending messages from one device to another. Ensure that messages are delivered promptly and accurately. | *Test ID:* 6 |
| *Version:* 1 | *Test Type:* Unit testing |
| *Input:* Message | |
| *Expected Result:* The message is successfully sent and is visible in user interface. | |
| *Actual Result:* Passed | |

**Description**: In this test case, user selects an IP address and sends a text message. The message was successfully sent and was visible on UI.

**Test Case 7: Testing that the message is successfully recieved by the android app**

**Table 5.7: Test Case 7**

|  |  |
| --- | --- |
| Date: 28 December 2023 |  |
| *System:* AndroCom |  |
| *Objective:* Confirm that the application receives and displays incoming messages correctly. Check for real-time updates and accuracy in displaying the sender's information. | *Test ID:* 7 |
| *Version:* 1 | *Test Type:* Unit testing |
| *Input:* None | |
| *Expected Result:* The message is successfully received and displayed on the UI. | |
| *Actual Result:* Passed | |

**Description**: In this test case, when the message was sent, it was successfully received by the android device and was displayed on the UI.

**Chapter 6**


**Software Deployment**

In this chapter, the entire installation process for the AndroCom app and microcontroller is provided. A detailed, step-by-step process is outlined on how the user can install the app on their Android device and set up their microcontroller for AndroCom. The user is required to have two things: an Android device and a Raspberry Pi, preferably newer than Raspberry Pi 4B. If a Raspberry Pi is unavailable, the user can emulate scripts on a Raspbian OS (Linux) supported device.


## 6.1 Installation / Deployment Process Description

**6.1.1 RaspberryPi Setup**

# To run the setup for Raspberry Pi, navigate to the terminal and use the command *"sudo ./setup\_hotspot.sh"* after locating the *"setup\_adhoc.sh"* file.




**Figure 6.1: Terminal in RaspbarianOS**



**Figure 6.2: Terminal in RaspbarianOS after successfully establishing AD HOC network**


Now, run the Python script that logs IP and MAC addresses and broadcasts them. Open the script in Thonny IDE and execute it.



**Figure 6.3: Thonny IDE in RaspbarianOS**


**6.1.2 Android Application**

On your Android device, enable developer options. Once enabled, activate wireless debugging and connect it with Android Studio.




**Figure 6.4: Wireless Debugging in Android Settings**

Open the **'AndroCom'** project folder in Android Studio. Once opened, connect your Android device via the device manager. Once connected, click on **"Build Project"**.



**Figure 6.5: Android Studio**

Once the project build is complete, the app will appear on the Android device.



**Figure 6.6: AndroCom App in Android Device's Home Screen**

References

**Book**

Kurose, J. F., & Ross, K. W. (2019). *Computer Networking: A Top-Down Approach* (8th edition). Pearson.

Griffiths, D., & Griffiths, D. (2017). *Head First Android Development*. O'Reilly Media.

**Webpage**

Google. (Updated regularly). Android Developers - Documentation. https://developer.android.com/. Accessed on January 18, 2024.

Python Software Foundation. (Updated regularly). Python Documentation. https://docs.python.org/3/. Accessed on January 1, 2024.

JetBrains. (Updated regularly). Kotlin Documentation. https://kotlinlang.org/docs/home.html. Accessed on January 04, 2024.

Oracle Corporation. (Updated regularly). Java SE Documentation. https://docs.oracle.com/en/java/javase/index.html. Accessed on January 04, 2024.